|  |  |  |
| --- | --- | --- |
| 17” - 19”430-485 mmWater Closet Height | 17” max430 mmWall Hung Urinal Height | 56” min, (59” min if floor-mount toilet)1420 mmOther fixtures not allowed within this area60” Min1525 mmSize of Clearance for Water Closet  |
| CL12” max305 mm16” – 18”430-485 mmAccessible Water Closets | 18” min455 mm39” – 41”990-1040 mm33” – 36”840-915 mm54” min1370 mm42” min1065 mm39” – 41”990-1040 mmSide Wall Grab Bar for Water Closet | Flush handle must be to wide side of lavatoryRear Wall Grab Bar for Water ClosetCL33” – 36”840-915 mm12” min305 mm24” min610 mm36” min915 mm |
| 42” max Protruding Dispenser Location: 24”min 1 ½" min18” min1. Below Grab Bar
 | Recessed Dispenser Location: 36” max24” min12” min1. Above Grab Bar

48” max | 42” max18” min36” max24” min48” max |

All dimensions per the

ANSI A117.1-2009 *and* the 2012 IBC Chapter 11 and Appendix E

|  |  |  |
| --- | --- | --- |
| 16”-18”405-455 mm56” min. (59” min. if floor –mount toilet)1420 mmMirrors located above lavatories, sinks or counters shall be mounted with the bottom edge of the reflecting surface 40” maximum above the floor30” Min760 mm60” Min1525 mmCL | Other fixtures NOT allowed within this areaClear floor space required at water closets and lavatories30” Min760 mm | 16”-18”405-455 mm56” min, (59” min. if floor-mount toilet)1420 mm48” Min1220 mm60” Min1525 mmCL |
| 17” min205 mmHeight of Lavatories & Sinks34” max865 mm | All pipes to be covered or wrapped40” max1016 mm | Mirrors not located above lavatories, sinks or counters shall be mounted with the bottom edge of the reflecting surface 35” maximum above the floor35” max889 mm |
| 8” min205 mmKnee and Toe Clearance – Sinks and Drinking Fountains6” max280 mm9” min230 mm11” min205 mm27” min685 mm | Drinking FountainSpout Location *Parallel Approach (only for children’s use)*48” min1219 mm30” min762 mm3 ½” max89 mm | 15” minCenterlineForward Approach 5” max125 mm15” min380 mm |