|  |  |  |
| --- | --- | --- |
| 17” - 19”  430-485 mm  Water Closet Height | 17” max  430 mm  Wall Hung Urinal Height | 56” min, (59” min if floor-mount toilet)  1420 mm  Other fixtures not allowed within this area  60” Min  1525 mm  Size of Clearance for Water Closet |
| CL  12” max  305 mm  16” – 18”  430-485 mm  Accessible Water Closets | 18” min  455 mm  39” – 41”  990-1040 mm  33” – 36”  840-915 mm  54” min  1370 mm  42” min  1065 mm  39” – 41”  990-1040 mm  Side Wall Grab Bar for Water Closet | Flush handle must be to wide side of lavatory  Rear Wall Grab Bar for Water Closet  CL  33” – 36”  840-915 mm  12” min  305 mm  24” min  610 mm  36” min  915 mm |
| 42” max  Protruding Dispenser Location:  24”min  1 ½" min  18” min   1. Below Grab Bar | Recessed Dispenser Location:  36” max  24” min  12” min   1. Above Grab Bar   48” max | 42” max  18” min  36” max  24” min  48” max |

All dimensions per the

ANSI A117.1-2009 *and* the 2012 IBC Chapter 11 and Appendix E

|  |  |  |
| --- | --- | --- |
| 16”-18”  405-455 mm  56” min. (59” min. if floor –mount toilet)  1420 mm  Mirrors located above lavatories, sinks or counters shall be mounted with the bottom edge of the reflecting surface 40” maximum above the floor  30” Min  760 mm  60” Min  1525 mm  CL | Other fixtures NOT allowed within this area  Clear floor space required at water closets and lavatories  30” Min  760 mm | 16”-18”  405-455 mm  56” min, (59” min. if floor-mount toilet)  1420 mm  48” Min  1220 mm  60” Min  1525 mm  CL |
| 17” min  205 mm  Height of Lavatories & Sinks  34” max  865 mm | All pipes to be covered or wrapped  40” max  1016 mm | Mirrors not located above lavatories, sinks or counters shall be mounted with the bottom edge of the reflecting surface 35” maximum above the floor  35” max  889 mm |
| 8” min  205 mm  Knee and Toe Clearance – Sinks and Drinking Fountains  6” max  280 mm  9” min  230 mm  11” min  205 mm  27” min  685 mm | Drinking Fountain  Spout Location    *Parallel Approach (only for children’s use)*  48” min  1219 mm  30” min  762 mm  3 ½” max  89 mm | 15” min  Centerline  Forward Approach  5” max  125 mm  15” min  380 mm |